FlySky FS-i6S Firmware Upgrade Steps:

**Version Updating:**

flysky i6s 1.10 22-Mar-2016 to flysky i6s 1.11 30-Jun

1. Need to bind with receiver again, 2. The menu set contents will be reset, please reset your transmitter.

flysky i6s 1.11 07-Jun-2016 to flysky i6s 1.11 30-Jun

Need to reset and calibrate the stick date. Please follow the calibration process to calibrate your transmitter.

**Upgrade Process:**

1. Connected the transmitter to the computer via USB cable.
2. Enter the Setup menu in the transmitter and navigate the Firmware Update section.
3. Open the firmware upgrade tool in your PC.
4. In the Firmware Update Section of the transmitter press Continue and the transmitter will enter the update mode.
5. Once the transmitter enters the update mode, you will see it listed in the software. Press Update in the software and the update process will begin. It should take a few seconds for the update to take place and then the transmitter will reboot.
6. Close the software and unplug the transmitter.
7. In the Setup section of the transmitter navigate to the About FS-i6S section to confirm the correct firmware.

**Calibration Process:**

Once the transmitter’s software has been successfully updated, it must be calibrated. Follow the following steps to calibrate your transmitter:

1. Enter the Setup menu and navigate to the Stick Adjust section to initiate the calibration process.
2. Simultaneously move both sticks up, down, left, right and then place the sticks at 50% or centered.
3. Move the two dials on the transmitter all the way left and right
4. Navigate to the Channels Section of the transmitter and verify that all the channels work accordingly.