**Standard wpa\_supplicant.conf for Kashmir Robotics Raspberry Pi**

ctrl\_interface=DIR=/var/run/wpa\_supplicant GROUP=netdev

update\_config=1

country=US

network={

        ssid="Kashmir50"

        psk="Kashmir1"

        key\_mgmt=WPA-PSK

}