**Streaming Video Gstreamer1.0**

On Raspberry Pi:

sudo modprobe bcm2835-v4l2

gst-launch-1.0 v4l2src device=/dev/video0 ! jpegenc ! rtpjpegpay ! udpsink host=10.0.0.140 port=9999  
  
\*10.0.0.140 is ip address for receiving computer  
  
  
gstreamer\1.0\x86\_64\bin>gst-launch-1.0.exe udpsrc port=9999 ! application/x-rtp,encoding-name=JPEG,payload=26 ! rtpjpegdepay ! jpegdec ! autovideosink  
  
• Port 9999 is same as on Raspberry Pi